*Press release*

*Saint-Blaise, 11 November 2014*

**Vertalor: the very essence of the watchmaker’s art**

*Ateliers Louis Moinet’s Vertalor is ushering in a new aesthetic era. Featuring a tourbillon with a cage hung beneath a three-armed gold bridge, it embodies the creative independence of the Ateliers, celebrating their tenth anniversary this year.*

**Creativity, unicity and authenticity are the Vertalor’s cardinal values**

The Vertalor expresses all the technical and aesthetic quintessence of Ateliers Louis Moinet, and is one of the finest expressions to date of what makes this independent *maison* based in Neuchâtel so singular. It also marks the first time that a tourbillon cage has hung from a three-armed bridge made from solid gold. The architectural theme of suspension continues with the Vertalor’s barrel, the cover of which also hangs from a gold bridge. Indeed, the gold bridge construction forms the backbone of the Vertalor – and heralds a completely new approach to open-dial watches.

The two series of Vertalors (28 in pink gold, 28 in grey gold) also embody the power of a design that has become the hallmark of Ateliers Louis Moinet: a sculpted case surrounding a dial revealing the technical beauty of the tourbillon. The latter is positioned at 6 o’clock and features a new hand whose tip, in the form of a luminous star, owes nothing to chance: it harks back to Mr Louis Moinet’s very own design for the Julius Caesar clock (1825).

**Curves and light**

At 12 o’clock these gold bridges make room for a more open, reworked barrel. Its cover features an open-work sun motif. At 6 o’clock, the tourbillon, hanging from the three bridges above, is suffused with light. Between the two, the winding cog can be seen, a witness to the human interaction with the crown and barrel that provides the watch with 72 hours’ power reserve.

The assembly is arrayed in an Ateliers feature that has become legendary: a broad dial embellished with a Côtes du Jura pattern. Two slightly curved open-work hands sweep across it, with the famous “Dew Drop” tips that have also become part of the brand’s aesthetic signature. A fragment of moon meteorite adorns the centre of the dial, at the centre of those distinctive hands.

At 9 o’clock rests the Fleur-de-lis, the emblem of Ateliers Louis Moinet. This completely redesigned, enlarged, mirror-polished applique detail denotes both Louis Moinet’s place in the course of history and his native town of Bourges (which displays the Fleur-de-lis on its coat of arms).

The eight curved, diamond-cut hour markers embody both technical prowess and a powerful aesthetic message – arching above the dial, they help to create a distinctive relief effect in this symbiosis of technology and design.

**Technical – and authentic**

In the very finest watchmaking tradition, the mechanical movement is manual wind. Set at 3 Hz, its generous three-day power reserve makes the Vertalor suitable for busy modern-day life. The assembly is firmly anchored to a distinctive case, designed and patented by Ateliers Louis Moinet, that is to be found in each of its collections. The case alone has no fewer than 59 parts. Front and back are made from sapphire glass, providing a breath-taking view of the hand-finished movement.

“*We wanted a timepiece that would pay tribute to Louis Moinet’s style, particularly that of the School of Fine Arts, where he taught on his return from Italy*,” explains Jean-Marie Schaller, CEO and Creative Director of the Ateliers. “*The Vertalor brings together the very essence of our present-day identity: it’s a radiant watch that highlights both technical achievement and the quest for aesthetic balance, complete with its Dew Drop hands, Côtes du Jura dial and many applique features. With such a wealth of details, producing this timepiece was especially exacting.”*

The 47mm-diameter Vertalor will be available in white gold and pink gold versions. Leading collectors have lost no time in taking possession of the first models.

:logo_585.jpg

***Louis Moinet turns ten!***

Visuals available at: <http://louismoinet.com/downloads.php>

Contact, interview requests, museum tours: [presse@louismoinet.com](mailto:presse@louismoinet.com)



LM-35.50.55

LM-35.70.50

**Technical specifications**

**Features and indications**

Exclusive tourbillon escapement

Central Hours and Minutes

Seconds

**Dial and hands**

Dial decorated with “Côtes du Jura” ®

18K gold three-armed bridge

Diamond-cut hour markers

Fragment of meteorite in the centre of the dial

“Gouttes de Rosée” (Dew Drop) hands marking hours and minutes

Luminous star-shaped second hand (Design inspired by Julius Caesar clock made by Louis Moinet in 1825)

**Movement and finishing**

Winding Manual

Mechanism visible through the case-back with “octopus” spring

Oscillations 21,600 vph

Frequency 3 Hz

Lines 14 ½

Power reserve 72 hours

Tourbillon cage One full rotation every 60 seconds

Jewels 19

Escapement Side lever

Decoration “Côtes du Jura” ® engraving, blued steel screws

**Case and strap**

Original design by Louis Moinet®, made up of 59 parts

Material 18K white gold

18K rose gold

Case diameter 47 mm

Water-resistance 30 metres

Caseback Secured with 6 screws, engraved with individual number and Louis Moinet markings

Crystals Two anti-reflective sapphire crystals

Strap Louisiana alligator leather, hand-sewn, width between lugs : 24 mm

Buckle 18k white gold (or 18K rose gold) folding clasp with Louis Moinet symbol

Presentation box Extra large Louis Moinet Book, hand-written warranty

Rarity Limited Edition of 28 pieces

Reference no. LM-35.70.50

LM-37.50.55